**Safety File Contents:**

1. **Safety File**
   1. **37.2.**
   2. **Public Liability.**
   3. **Letter of Good Standing.**
   4. **Copies of Employees ID’s, License for construction vehicles and skilled training certificates.**
   5. **All Building Regulations of South-Africa and by Laws.**
   6. **Step Ladders must be SABS Approved.**
   7. **Scaffolding to be inspected and signed off by Safety Officers.**
   8. **Service Records must be displayed of compressors and Generators.**
2. **Basic PPE (Persona Protective Equipment).**
3. **Presentation of Technical drawings for designer stands.**
4. **Rigging Engineer Certificate (COC) after erecting of the design.**
5. **Structural Engineer Certificate (COC) after erecting of the design.**
6. **Electrical Engineer Certificate (COC) after erecting of the design.**
7. **All draping to be fire treated with certificate not older than 14 days.**
8. **Food & Catering (COA) Certificate to be displayed.**

**Double story designs**

1. **NO Spiral steps allowed.**
2. **Railings on steps.**
3. **White Photo luminous strips on edges of steps.**
4. **Photo luminous sign by entrance of steps saying max people allowed 25 pax.**
5. **Exceeding of 25 pax will need 2 entrances, same rules comply.**
6. **Fire extinguisher per entrance.**
7. **Minimum of 2 smoke detectors on roof.**
8. **Carpets to be fire treated.**
9. **Compressed wood must comply with fire ratings certificate.**